Cmp-Mod V01 Created by CvPCB (2011-03-30 BZR 2932)-stable date = lun. 10 juin 2013 17:05:05 CEST

BeginCmp
TimeStamp = /502E492C;
Reference = BT1;
ValeurCmp = 1,5V_ou_3V;
IdModule  = SIL-2;
EndCmp

BeginCmp
TimeStamp = /502E47EF;
Reference = C1;
ValeurCmp = 10n;
IdModule  = C2;
EndCmp

BeginCmp
TimeStamp = /502E4862;
Reference = C2;
ValeurCmp = 10u_16V;
IdModule  = C1V5;
EndCmp

BeginCmp
TimeStamp = /502E49AC;
Reference = C3;
ValeurCmp = 10u_16V;
IdModule  = C1V5;
EndCmp

BeginCmp
TimeStamp = /502E4AA8;
Reference = C4;
ValeurCmp = 10u_16V;
IdModule  = C1V5;
EndCmp

BeginCmp
TimeStamp = /502E47D7;
Reference = D1;
ValeurCmp = 1N4148;
IdModule  = D4;
EndCmp

BeginCmp
TimeStamp = /502E47DC;
Reference = D2;
ValeurCmp = 1N4148;
IdModule  = D4;
EndCmp

BeginCmp
TimeStamp = /5034D408;
Reference = J0;
ValeurCmp = JACK_STEREO;
IdModule  = Jack3_5_Stereo_F126-7376-simple-face;
EndCmp

BeginCmp
TimeStamp = /502E4A81;
Reference = J1;
ValeurCmp = JACK_STEREO;
IdModule  = Jack3_5_Stereo_F126-7376-simple-face;
EndCmp

BeginCmp
TimeStamp = /502E48B1;
Reference = P1;
ValeurCmp = BNC_ou_Bornier;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /502E480C;
Reference = Q1;
ValeurCmp = NPN_faible_bruit;
IdModule  = TO92-123;
EndCmp

BeginCmp
TimeStamp = /502E4811;
Reference = Q2;
ValeurCmp = BC547B;
IdModule  = TO92-123;
EndCmp

BeginCmp
TimeStamp = /502E4818;
Reference = Q3;
ValeurCmp = BC547B;
IdModule  = TO92-123;
EndCmp

BeginCmp
TimeStamp = /502E4849;
Reference = R1;
ValeurCmp = 10k;
IdModule  = R5;
EndCmp

BeginCmp
TimeStamp = /502E49CA;
Reference = R2;
ValeurCmp = 100k;
IdModule  = R5;
EndCmp

BeginCmp
TimeStamp = /502E483E;
Reference = R3;
ValeurCmp = 10k;
IdModule  = R5;
EndCmp

BeginCmp
TimeStamp = /502E49B4;
Reference = R4;
ValeurCmp = 100k;
IdModule  = R5;
EndCmp

BeginCmp
TimeStamp = /502E4835;
Reference = R5;
ValeurCmp = 1k;
IdModule  = R5;
EndCmp

BeginCmp
TimeStamp = /51AC8A50;
Reference = SW1;
ValeurCmp = PUSH_SW;
IdModule  = PUSH_SW_GE;
EndCmp

EndListe
